**PONDICHERRY UNIVERSITY**

**ENGINEERING WING**

**Schedule of Work**

**Name of work:** Supplying and installation of furniture to the newly constructed

building for MSGET and Bio-Informatics

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **S.**  **No.** | **Description** | **Qty** | **Rate**  **Rs.P.** | **Unit** | **Amount**  **Rs.P.** |
| 1 | Conference table of size 300x90x75cm, (comprises of 2 part) made of 18mm thick commercial plywood with 1mm thick teak colour matt mica finish one row utility shelf around the table | 4 |  | Each |  |
| 2 | Conference chair made of teak wood of front breadth 59cm, height 37cm, back side breadth 59cm, height 64cm, side breadth 56cm, round leg 6cm dia. All cross reaper 4x2cm, handle 6x2 cm, “U” foam seat thick 9cm. Back thick 7cm, of quality 32 density, with 18mm commercial plywood. | 48 |  | Each |  |
| 3 | Auditorium chair for seminar hall. (specification of chairs are enclosed) | 250 |  | Each |  |
| 4 | Dual desk made of teak wood, desk top and bench seat and back 18 mm thick commercial plywood with 1mm thick teak colour matt (mica) finish, book shelf only 12mm thick commercial plywood with 1mm thick matt mica finish, Table size 120x45x80/78 cm. And 120x37x45/90cm, teak wood leg size 4.5x4.5cm, desk top cross reaper 11x2 cm, desk bottom cross reaper 4.5x2cm, bench seat rest top and bottom cross reaper 4.5x2cm, back rest top reaper 7x2cm, and 4.5x2cm, bottom base frame with 7x3cm size 2 nos and 4.5x3cm size 2 nos. all plywood bottom of golden brown paint finish. | 101 |  | Each |  |
| 5 | Lab table made of teak wood of size 150x75x90cm with 2 drawers and 8 cupboards with doors, leg size 6x6cm top cross reaper 12x3cm drawer side top reaper 4.5x3cm bottom and all other cross reapers 6.5x3cm. Table top made of 15mm thick granite top. Table bottom and shelf plank are 1.8 cm thick with 5 joints and drawers all side plank are 1.8 cm thick. All side planks including door plank made of 1cm thick plank, drawer bottom with 8 mm commercial ply with 0.8mm mica finish. Drawer size 60x55x14cm and door pad lock arrangement with one reagent rack of size 140x15x52cm made of 18mm thick teak wood plank with polish finish. | 41 |  | Each |  |
| 6 | Stool made of teak wood of size 37x37x51 cm, leg size 4.5x4.5cm, all cross reaper 4.5x2cm, top plank 2cm thick with one joint two planks. | 115 |  | Each |  |
| 7 | Executive office table of size 210x90x75 cm right side 3 drawer and left side shelf attached with 5mm glass sliding door, inner side ivory color paint finish top made of 35mm thick commercial plywood, drawer bottom 6mm commercial plywood with 0.8mm thick teak color matt mica finish, round leg of 6mm diameter, drawer side plank 1.5cm thick in teak wood, drawer size 60x39x12 cm with locking arrangements. | 2 |  | Each |  |
| 8 | Assistant table made of teak wood of size 120x75x75cm, leg size 4.5x4.5cm. Top cross reaper 7x2cm, foot rest reaper 7x3cm, Bottom side reaper 4.5x3cm, right side with one drawer and cupboard of size 60x40x60cm, made of 18mm commercial plywood with 1mm thick teak colour matt mica finish. Table top 18mm plywood with 1mm mica (matt) finish, Drawer size 55x36x11cm, drawer side plank 1.5cm thick drawer bottom 6mm commercial plywood with 1mm thick teak colour matt mica finish with locking arrangement. | 9 |  | Each |  |
| 9 | Teachers desk (120x60x75cm) made of 18mm commercial ply with three drawers made of 1.8cm thick teak wood plank and locking arrangements | 5 |  | Each |  |
| 10 | Assistant chair Seat and back nylon knitted in teak wood front leg 4.5x4.5cm, back leg, top and bottom 3x3cm, center part 4x3cm, handle and back rest top reaper of 7x2cm, handle length 58cm, seat rest frame reaper of size 4.5x3cm, bottom support reaper 4x2cm, front height (seat) 45cm handle level at height 68 cm, breath 56cm, back height 90cm. breadth 46cm, side breadth 52cm. | 95 |  | Each |  |
| 11 | Steel computer revolving chair standard size, seat and back cushion with arms and push back arrangement and height adjustable. | 200 |  | Each |  |
| 12 | Teak wood sofa set three seater 1 no. single seater 2nos. each with 65x30mm legs and outer frame, inner reaper 45x30mm thick reaper, filled at a intervening distance of 40mm in seat and back with 3 detachable 100mm foam seat and 3 detachable 75mm thick. | 1 |  | Each |  |
| 13 | Steel cupboard with 4mm glass panels in the doors made of 1mm thick 20 gauge CR sheet size 195x90x48cm (4 shelves and 5 compartments). | 2 |  | Each |  |
| 14 | Cupboard made of 18mm commercial ply with mica finish, door with 4mm plain glass of size 180x30x60cm. (4 shelves and 5 compartments). | 6 |  | Each |  |
| 15 | Maruthi Inspace Modular workstations of size 750(W) x 525(D) x 1200(H) of self supporting partition @ thickness of 75mm base steel frame vertical section made out of 18 SWG(1.2mm) CRCA steel framed into channels duly powder coated @ 50 microns. Tiles are made out of 9mm thick pre-laminated particle board for top and bottom. Privacy partition glass fixed on work top @ 4mm thick plain glass. Separate race way @ 150mm thick at bottom level for cable management made out of 18 SWG (1.2 mm) CRCA steel. Top cover made out of curved aluminium extruded section with powder coated finish. Corner posts are made out of 1.6mm thick MS Cr Tubular section with powder coated finish. Work top/ side panels (legs) fabricated out of 25mm thick PLB duly edge banded with 2mm thick PVC beading .Accessories: Keyboard tray size 600x300mm made out of 18mm thick pre-laminated particle board with laminated on both sides with 2mm thick PVC edge banded both sides fixed sliding channels for easy movement CPU trolley-Made out of MS sheet with powder coated. CPU trolley with lockable wheels. | 165 |  | Each |  |
| 16 | Supplying and fixing of Ceramic white marker board of make Alkosign (4’X 10’). | 7 |  | Each |  |
| 17 | Supply of steel visitor chair seat and back cushion with ABS low back rest with arms. Steel pipe portion powder coated | 32 |  | Each |  |
| 18 | Dual desk (three seater) made of teak wood, desk size: 150x45x80/78 cm, Bench size:150x37x90/45 cm, legs size:4.5x4.5 cm, Desk top side reaper 14.2 cms, bottom side cross reaper 4.5x2 cms, bench back rest top reaper 7x3 cm, Bench seat support and back rest middle reaper 4.5x3cms, bottom side reaper 4.5x2cms bench and desk connected bottom support frame reaper 7x3 cm-2Nos and 4.5x3 cm- 2Nos. Bench seat and Back , Desk table top 18mm commercial plywood with 1 mm thick teak colour matt mica finish, Desk book shelf made of 12mm commercial plywood with 1mm thick teak colour matt mica finish, book shelf side inner and plywood back side golden brown paint finish. | 6 |  | Each |  |
| 19 | Fume hood cupboard (Visvam brand) of size 135x75x165cm made of teak wood with mica finish, top part all four sides closed with 5mm polycarbonate sheets with front side 5mm polycarbonate sliding door, top working chamber top and bottom with 12mm nylon sheet fixing, bottom cupboard with shelf made of teak wood, fume hood bottom shelf and bottom part top made of 2cm thick teak plank with joint. Bottom part storage chamber provided with teak wood double door, bottom exhaust chamber with single door. Right side of the fume hood provided with 3 sets of 15A switch and socket. Teak wood doors without locks and with magnetic catches. Leg size 6x6 cm, All cross reaper 7x3cm. | 9 |  | Each |  |
| 20 | Individual students chair (single seater) made of teak wood armless chair, size 44x46x90/45 cm, leg size 4.5x4.5 cm, chair cheat made of 18mm commercial ply with 1mm mica finish. | 70 |  | Each |  |
| 21 | Executive revolving chair Hi Back, seat and back cushion with arms and push back arrangement and height  adjustable. | 5 |  | Each |  |
| 22 | Reagent rack of size 105x20x50 cm, made of 18mm water proof plywood with light green(Pista colour ) paint finish front side 5mm glass sliding door, back side 8mm water proof plywood (2shelves and 3 compartments). | 15 |  | Each |  |
| 23 | Over head storage of size 750(L)x375(w)x450(h)-swing door fabricated out of 18mm thick pre-laminated particle board duly edge banded with 2mm thick PVC beading and provided doors fixed with butterfly hinges with handles and locks (1shelve and 2 compartments). | 14 |  | Each |  |
| 24 | Steel almirah made of 1mm thickness CR sheet (20 Guage) with 4 shelves making 5 compartment without locker, size :1980x915x485 mm | 25 |  | Each |  |
| 25 | File cabinet (four drawer) made of 1mm thick 20 gauge CR sheet (size 137x70x47cm) | 9 |  | Each |  |
| 26 | Computer table of size 120x45x75 cm made of 18mm thick commercial plywood with 1mm thick beach colour matt mica finish drawer bottom 6mm thick commercial plywood with 0.8mm thick matt mica finish with locking arrangements left side one drawer right side key board | 14 |  | Each |  |
| 27 | Wet lab table: size 150x75x90cm made of 18mm ply with 1mm thick mica finish, right side one drawer with cupboard, back side 12mm ply, bottom base 7x3 cm in teak wood and one reagent rack of size 150x30x75 cm made of 18mm ply with 1mm thick mica finish with 5mm glass sliding door, back side 12 mm ply, front side with combined 15 A and 5A switch and socket-4nos over 3mm for mica sheet, all sides except backside with mica finish, backside alone with paint finish. Table top made of 18mm ply with 15mm thick granite. Drawer bottom made 8mm ply with mica finish. | 20 |  | Each |  |
| 28 | Wet lab table: size 180x60x90cm made of 18mm ply with 1mm thick mica finish, right side one drawer with cupboard, back side 12mm ply, bottom base 7x3 cm in teakwood, all sides except backside with mica finish, backside alone with paint finish. Table top made of 18mm ply with 15mm thick granite. Drawer bottom made 8mm ply with mica finish. | 8 |  | Each |  |
| 29 | Instrument lab table: : size 150x60x90cm made of 18mm ply with 1mm thick mica finish, right side one drawer with cupboard, back side 12mm ply, bottom base 7x3 cm in teakwood, all sides except backside with mica finish, backside alone with paint finish. Table top made of 18mm ply with 15mm thick granite. Drawer bottom made 8mm ply with mica finish. | 3 |  | Each |  |
| 30 | Instrument lab table with sink: size 150x60x90cm made of 18mm ply with 1mm thick mica finish, right side one cupboard, back side 12mm ply, bottom base 7x3 cm in teakwood, all sides except backside with mica finish, backside alone with paint finish. Table top made of 18mm ply with 15mm thick granite. | 2 |  | Each |  |
| 31 | Research lab table: size 180x75x90cm made of 18mm ply with 1mm thick mica finish, right side one drawer with cupboard, back side 12mm ply, bottom base 7x3 cm in teak wood and one reagent rack of size 150x30x75 cm made of 18mm ply with 1mm thick mica finish with 5mm glass sliding door, back side 12 mm ply, front side with combined 15 A and 5A switch and socket-4nos over 3mm for mica sheet, all sides except backside with mica finish, backside alone with paint finish. Table top made of 18mm ply with 15mm thick granite. Drawer bottom made 8mm ply with mica finish. | 13 |  | Each |  |
| 32 | Dias Teapoy made of teak wood of size:90x45x45 cm, leg size 4.5x4.5 cm, top cross reaper 7x2cm, bottom cross reaper 3x2cm, top 18mm plywood with 1mm teak colour matt mica finish, bottom 8mm plywood with 1mm thick mica finish | 2 |  | Each |  |
| 33 | Podium made of teak wood of size 50x45x116 cm with two turned legs of size 7 x 7cm with 4mm acrylic sheet between legs for display purpose. | 2 |  | Each |  |
| 34 | Steel rack 18 Guage sheet and32x32x4mm angle of 4 shelves 3 compartments rigid type- non- adjustable shelves, size 1980x915x405mm. | 1 |  | Each |  |
|  | **Total** |  |  |  |  |

I hereby abide by the rules & regulations stipulated in the CPWD form no.6 & 8

**Contractor Registrar**